; sertouch.inf
;
; Installation file (.inf) for the eGalaxTouch device.
;
; (c) Copyright 2000 ~ 2012 Inc. 
;

[Version]
Signature="$Windows NT$"
Provider=%EGALAXTOUCH%
ClassGUID={4D36E96F-E325-11CE-BFC1-08002BE10318}
Class=Mouse
CatalogFile=sertouch.cat
DriverVer=12/01/2012, 5.12.0.11001
[SourceDisksNames]
1 = %DiskId1%,,
[DestinationDirs]
DefaultDestDir   = 12
DLLCopyFiles = 11
;
; Driver information
;

[Manufacturer]
%EGALAXTOUCH%   = eGalaxTouchMfg, NTamd64 ;

[eGalaxTouchMfg.NTamd64]
%SERTOUCH_PNP%       = sertouch_Inst.x64, SERENUM\EGX5800
%SERIAL_LEGACY%	     = sertouch_Inst.x64, SERENUM\EGX5900
%SERIAL_COMBUS%	     = sertouch_Inst.x64, SERENUM\EGX6000

;
; General installation section
;
; ======= Serial Touchscreen Section ====================
[sertouch_Inst.x64]
AddReg=sertouch_AddReg.x64
; Copy the driver over
CopyFiles=SerCopyFiles_Drivers.x64, DLLCopyFiles.x64

[sertouch_AddReg.x64]
;
; File sections
;
;HKR,,EnumPropPages32,,"SerTKProp.dll,EnumPropPages"

[SerCopyFiles_Drivers.x64]
sertouch.sys

[DLLCopyFiles.x64]
;SerTKProp.dll
;
; Service Installation
;

[sertouch_Inst.x64.HW]
DelReg = sertouch_DelReg.x64
AddReg = sertouch_Inst_AddReg.x64

[sertouch_Inst.x64.Services]
AddService = sertouch, 0x00000002 , sertouch_Service_Inst.x64, sertouch_EventLog_Inst.x64
; Install mouclass.sys from msmouse.inf
Include=msmouse.inf
Needs=MouClass.Services

[sertouch_Service_Inst.x64]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 0                  ; SERVICE_ERROR_IGNORE
LoadOrderGroup = Pointer Port
ServiceBinary  = %12%\sertouch.sys

[sertouch_EventLog_Inst.x64]
AddReg = sertouch_EventLog_AddReg.x64

[sertouch_EventLog_AddReg.x64]
HKR,,EventMessageFile,0x00020000,"%SystemRoot%\System32\IoLogMsg.dll;%SystemRoot%\System32\drivers\sertouch.sys"
HKR,,TypesSupported,0x00010001,7

[sertouch_Inst_AddReg.x64]
;HKR,,"BeepMode",0x00010003,1
;HKR,,"MouseMode",0x00010003,0x00000000

[sertouch_DelReg.x64]
;HKR,,"BeepMode"
;HKR,,"BeepFrequency"
;HKR,,"BeepDuration"
;HKR,,"MouseMode"
;HKR,,"ConstDuration"
;HKR,,"ConstMode"
;HKR,,"ConstRange"
;HKR,,"EdgeInfo"
;HKR,,"Branch"
;HKR,,"CalInfo"
;HKR,,"CalSource"
;HKR,,"LinzInfo"
;HKR,,"Migrated"
;HKR,,"MonitorInfo"
;HKR,,"NativeName"
;HKR,,"Orient"
;HKR,,"SymbolicName"
;HKR,,"TouchGrid"
;HKR,,"TouchSpeed"


[SourceDisksFiles]
; Files for disk eGalaxTouch Touchscreen Controller. Installation Disk #1 (Mouse)
sertouch.sys = 1,,
;egxfilter.sys = 1,,


[Strings]

;
; Non-Localizable Strings
;

REG_SZ         = 0x00000000
REG_MULTI_SZ   = 0x00010000
REG_EXPAND_SZ  = 0x00020000
REG_BINARY     = 0x00000001
REG_DWORD      = 0x00010001
SERVICEROOT    = "System\CurrentControlSet\Services"

;
; Localizable Strings
;
SERTOUCH_PNP 	= "Serial Touchscreen Controller x64(Professional)"
SERIAL_LEGACY	= "Serial Touchscreen Controller x64"
SERIAL_COMBUS = "Serial Touchscreen Controller x64(ComBus)"
DiskId1 = "eGalaxTouch. Driver Installation Disk(TouchScreen)"
EGALAXTOUCH = "eGalaxTouch"
